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	Product information
	A water-based acrylic primer for walls and floors, specifically designed for damp surfaces prone to fungi and mold. It acts as a bonding agent and is ideal for preparing compatible substrates before the direct installation of flooring and wall coverings.

· Exceptional coverage
· Easy to apply
· Water-based and solvent-free
· Ideal for preparing surfaces that need to be leveled
· Binds residual dust
· Seals mortar pores, improving the fluidity and workability of self-leveling compounds
· Creates strong bonding bridges
· High yield
· Non-flammable
· Penetrates up to 3 cm into the substrate, consolidating it
· Very low VOCs (Volatile Organic Compounds)

	Recommended uses
	· Restoring old walls.
· Protecting and preventing fungi and molds on wet walls.
· PRIMER STO-SP prepares the wall surface before applying wall coverings and paints.

	Coverage
	[bookmark: _Hlk102401543]Approximately 75 square feet per quart, depending on the porosity of the substrate.

	Application instructions
	[bookmark: _Hlk102554440]Product preparation
The product is ready to use. 
The application substrate must meet the compatibility requirements of the Primer. They must be clean, free of structural defects, stationary, permanently dry and free of release agents. In the case of cementitious substrates, any retention must be removed by special machines.

Application
Shake well before use. Apply PRIMER STO-SP to walls or floors using a roller or brush, ensuring that no puddles form.  The product typically dries within 3 to 4 hours at 68–73°F (20–23°C), after which wallpaper can be applied. Drying time may vary depending on temperature, relative humidity, and substrate absorbency. Full drying time is approximately 48 hours.
On particularly porous surfaces, a second coat may be necessary. Drying time is influenced by the relative humidity and absorbency of the substrate; it will be shorter in higher temperatures and lower humidity, but longer in lower temperatures, higher humidity, and with non-absorbent substrates.                                                                                                                                                                                                                                                          

Cleaning
Clean any spills with a damp sponge. 
THE PRODUCT DOES NOT STAIN




	Technical product data

	Base
	Water-based acrylic

	
	Appearance and color 
	White liquid

	
	pH
	6.5

	
	Viscosity
	500-700 cps 

	
	VOC
	<2 µg/m3

	
	Solids percentage
	50 %

	
	Customs code 
	3209 1000

	
	Application temperature
	+41°F-+104°F

	
	Full drying time
	48 hours

	
	Non-flammable product
	

	
	Protect from freezing
	

	Warning
	Do not apply on non-absorbent substrates (glass, ceramic, laminates). Protect from frost.  Do not install floor coverings at temperatures below 59°F (15 ºC) and above 122°F (50 ºC) or at a relative humidity above 75 %. Do not mix PRIMER STO-SP with other primers. Do not apply to wood substrates. Do not add additional water.                            


	Storage

	The product is guaranteed in its original packaging, in standard conditions +41°F to + 95°F (+5 °C to + 35 °C), for 24 months from date of production. It is important to keep the product in dry conditions, away from heat sources and direct sunlight.

	[bookmark: _Hlk102401875]Disclaimer

	PRIMER STO-SP is free of solvents, lead or other heavy metals and is a suitable alternative to products containing solvents. No special safety precautions are necessary when working with the product, however personal protective equipment should be used as rubber gloves for industrial use, goggles and a dust mask. The risk of medium or long-term release of appreciable concentrations of volatile organic chemicals (VOCs) into ambient air is insignificant. However, ensure adequate ventilation during and after application and drying. Avoid eating, drinking or smoking while working with the product.
Protect eyes and skin. In case of contact with eyes or skin rinse immediately with plenty of water. After contact also consult a doctor.
The information contained in this data sheet, although based on our extensive experience, is for guidance only. Users must assess whether the product is suitable for the intended application and assume responsibility for its use.
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